
Version1.0.0.15
---------------
Note:The following parameters need to be added like this in mosusbce.reg file to vary,
As default-damping interval is 20 seconds for disconnect and 10 seconds for connect.
 [HKEY_LOCAL_MACHINE\Comm\mosusbce1\Parms\TcpIp]
"ConnectDampingInterval"=dword:1
"DisconnectDampInterval"=dword:2 ;If DHCP 10 
-------------------------------------------------------------------
1.Please do apply the "Moschip zero length patch" if EHCI host controller is used for MCS7830 device for WinCE 6.0
2.To apply the EHCI patch follow the "StepsToFixEHCIIssue.doc" 
3.To install the MCS7830 driver follow the "MosUsbCe InstallationNotes.doc"